LF353
Dual JFET-input operational amplifiers.

     +----------+
1OUT |1  +--+  8| VCC
-1In |2        7| 2OUT
+1In |3 LF353  6| -2In
 VEE |4        5| +2In
     +----------+

[This information is part of the GIICM]

